{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["MMVAL V1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"MMVAL V1","index":0,"n_rows":28,"n_cols":12,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Parça","FULL","MIKTAR","REFERANS","DEĞER","ALT","KILIF","MontajTipi","Sağlayıcı","ParçaNo","CCODE","  Revised: Tuesday, November 09, 2010"]
[1,"VAR",1,"BT1","3V_TH_CEP + 2032 PIL","--","CONCOINCELLCR2032THMNEW","TH","--","--","C1"]
[2,"VAR",1,"CON1","microSD_3M","--","MICRO_SD_3M","SMD","DIGIKEY","2908-05WB-MG","C2"]
[3,"VAR",1,"CON2","SD_CARD","--","SDCARDCONNMOLEX","SMD","DIGIKEY","67600-8002","C3"]
[4,"--",1,"CON3","SAM1","--","SIMCARDCONNECTOR6LI_NEW","SMD","--","--","C4"]
[5,"VAR",1,"CON4","SAM1","--","SIMCARDCONNECTOR6LI_NEW","SMD","--","--","C5"]
[6,"VAR",10,"C1,C6,C80,C81,C82,C83,C87,C88,C89,C90","10n","--","SMC0603","SMD","--","--","C6"]
[7,"VAR",1,"C2","470u/10V","--","SMCSMD83X83","SMD","--","--","C7"]
[8,"VAR",45,"C3,C5,C9,C15,C17,C19,C21,C22,C31,C37,C40,C41,C48,C51,C53,C55,C60,C63,C70,C103,C104,C105,C106,C107,C108,C109,C110,C111,C112,C113,C114,C115,C116,C117,C118,C119,C125,C129,C133,C142,C143,C144,C145,C147,C148","100n","--","SMC0603","SMD","--","--","C8"]
[9,"VAR",1,"C4","220u/>35V","220u/>35V","SMCSMD83X83","SMD","--","--","C9"]
[10,"VAR",1,"C7","470u/>16V","--","SMCSMD83X83","SMD","--","--","C10"]
[11,"VAR",2,"C8,C11","220u/>35V","100u/>35V","SMCSMD83X83","SMD","--","--","C11"]
[12,"VAR",1,"C10","470u/>10V","470u/>10V","SMCSMD83X83","SMD","--","--","C12"]
[13,"VAR",1,"C12","22n","--","smc0603","SMD","--","--","C13"]
[14,"VAR",1,"C13","220p","--","SMC0603","SMD","--","--","C14"]
[15,"VAR",1,"C14","DNP","--","SMC0603","SMD","--","--","C15"]
[16,"VAR",20,"C16,C18,C20,C42,C43,C44,C47,C52,C54,C56,C59,C76,C77,C78,C79,C85,C86,C93,C94,C149","10u","--","SMC0805","SMD","--","--"]
[17,"--",10,"C23,C26,C29,C33,C73,C99,C100,C101,C139,C140","100n","--","SMC0603","SMD","--","--"]
[18,"--",2,"C24,C25","22p","--","SMC0603","SMD","--","--"]
[19,"--",9,"C27,C32,C34,C121,C123,C124,C128,C131,C132","220n","--","SMC0603","SMD","--","--"]
[20,"--",2,"C28,C30","10u","--","SMC0805","SMD","--","--"]
[21,"--",2,"C35,C36","22n","--","SMC0603","SMD","--","--"]
[22,"VAR",2,"C38,C39","15p","--","SMC0603","SMD","--","--"]
[23,"VAR",3,"C45,C49,C146","10u/6V3/CER","--","SMC0805","SMD","--","--"]
[24,"VAR",2,"C46,C50","100n","--","SMR0603","SMD","--","--"]
[25,"VAR",8,"C57,C58,C61,C62,C65,C66,C68,C69","220n","--","SMC0805","SMD","--","--"]
[26,"VAR",2,"C64,C67","27p","--","SMC0603","SMD","--","--"]
[27,"--",2,"C71,C72","15p","--","SMC0603","SMD","--","--"]